From: <Saved by Windows Internet Explorer 8>
Subject: Serial In - Parallel Out Shift Registers
Date: Sat, 1 Jan 2011 15:25:11 +0200
MIME-Version: 1.0
Content-Type: multipart/related;
	type="text/html";
	boundary="----=_NextPart_000_01C8_01CBA9C8.14AF57A0"
X-MimeOLE: Produced By Microsoft MimeOLE V6.00.2900.5994

This is a multi-part message in MIME format.

------=_NextPart_000_01C8_01CBA9C8.14AF57A0
Content-Type: text/html;
	charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable
Content-Location: http://www.eelab.usyd.edu.au/digital_tutorial/part2/register03.html

<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0 Transitional//EN">
<HTML><HEAD><TITLE>Serial In - Parallel Out Shift Registers</TITLE>
<META content=3D"text/html; charset=3Diso-8859-1" =
http-equiv=3DContent-Type><!-- Created with AOLpress/2.0 -->
<META name=3DGENERATOR content=3D"MSHTML 8.00.6001.18975"></HEAD>
<BODY link=3D#808000 bgColor=3D#ffffff vLink=3D#ff80c0>
<P align=3Dcenter><IMG border=3D0 alt=3DRegisters=20
src=3D"http://www.eelab.usyd.edu.au/digital_tutorial/part2/pics/register0=
1s.gif"=20
width=3D200 height=3D60>=20
<H1 align=3Dcenter><FONT color=3Dteal><I>Serial In - Parallel =
Out<BR>Shift=20
Registers</I></FONT> </H1>
<BLOCKQUOTE><B>For this kind of register, data bits are entered serially =
in=20
  the same manner as discussed in the last section. &nbsp;The difference =
is the=20
  way in which the data bits are taken out of the register. &nbsp;Once =
the data=20
  are stored, each bit appears on its respective output line, and all =
bits are=20
  available simultaneously. &nbsp;A &nbsp;construction of a <FONT=20
  color=3D#ff0080>four-bit serial in - parallel out register </FONT>is =
shown=20
  below.</B> </BLOCKQUOTE>
<P align=3Dcenter><IMG border=3D0 alt=3D"4-bit SIPO register"=20
src=3D"http://www.eelab.usyd.edu.au/digital_tutorial/part2/pics/regist03.=
jpg"=20
width=3D452 height=3D156><BR>
<BLOCKQUOTE><B>In the animation below, we can see how the four-bit =
binary=20
  number 1001 is shifted to the Q outputs of the register.</B> =
</BLOCKQUOTE>
<P align=3Dcenter><IMG border=3D0 alt=3D"4-bit SIPO animation"=20
src=3D"http://www.eelab.usyd.edu.au/digital_tutorial/part2/pics/4sipo0.gi=
f"=20
width=3D235 height=3D40><BR>
<P><BR><BR>
<P align=3Dcenter><IMG border=3D0=20
src=3D"http://www.eelab.usyd.edu.au/digital_tutorial/part2/pics/bhf_g.gif=
" isMap=20
width=3D300 height=3D40 useMap=3D#bhfr><MAP name=3Dbhfr> <AREA=20
  =
href=3D"http://www.eelab.usyd.edu.au/digital_tutorial/part2/register04.ht=
ml"=20
  shape=3DRECT coords=3D200,0,300,40><AREA=20
  =
href=3D"http://www.eelab.usyd.edu.au/digital_tutorial/part2/hpage.html"=20
  shape=3DRECT coords=3D102,0,200,40><AREA=20
  =
href=3D"http://www.eelab.usyd.edu.au/digital_tutorial/part2/register02.ht=
ml"=20
  shape=3DRECT coords=3D0,0,102,40></MAP><BR><BR></P></BODY></HTML>

------=_NextPart_000_01C8_01CBA9C8.14AF57A0
Content-Type: image/gif
Content-Transfer-Encoding: base64
Content-Location: http://www.eelab.usyd.edu.au/digital_tutorial/part2/pics/register01s.gif

[encoded data, 4332 characters]
A4RCeITvR4NIuIR+syU7yIRQ+DYBAQA7

------=_NextPart_000_01C8_01CBA9C8.14AF57A0
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: http://www.eelab.usyd.edu.au/digital_tutorial/part2/pics/regist03.jpg

[encoded data, 14668 characters]
Tq9WXl9CFhSmnGoYSsA/lO1gHB7OBB9xFblKUClKUH//2Q==

------=_NextPart_000_01C8_01CBA9C8.14AF57A0
Content-Type: image/gif
Content-Transfer-Encoding: base64
Content-Location: http://www.eelab.usyd.edu.au/digital_tutorial/part2/pics/4sipo0.gif

[encoded data, 6688 characters]
TFZJRVdcc2lwbzQuZ2lmAAA7

------=_NextPart_000_01C8_01CBA9C8.14AF57A0
Content-Type: image/gif
Content-Transfer-Encoding: base64
Content-Location: http://www.eelab.usyd.edu.au/digital_tutorial/part2/pics/bhf_g.gif

[encoded data, 38604 characters]

------=_NextPart_000_01C8_01CBA9C8.14AF57A0--
